2007 INFINITI FX45/FX35 Specifications
Specifications are based on latest product information available at the time of printing.



2007 INFINITI FX45/FX35 Specifications

janvier 1, 2007




Engine
 FX45 
 FX35 



&nbsp;
&nbsp;
&nbsp;


Type
VK45DE DOHC 32-valve
VQ35DE DOHC 24-valve


Orientation
Longitudinal
Longitudinal


Cylinders / configuration
V8 with molybdenum coated pistons
V6 with molybdenum coated pistons


Block/head
Aluminum/ aluminum
Aluminum/ aluminum


Displacement
4.5 litres
3.5 litres


Horsepower
315 hp @ 6,400 rpm
280 @ 6,200 rpm


Torque
329 ft-lbs @ 4,000 rpm
270 ft-lbs @ 4,800 rpm


Bore x stroke (mm)
93.0 x 82.7
95.5 x 81.4


Compression ratio (:1)
10.5
9.3


Valvetrain
Four titanium valves per cylinder with continuous variable valve timing control
Four valves per cylinder with continuous variable valve timing control


Recommended fuel
Premium 
unleaded
Premium 
unleaded


Max. engine speed
6,600 rpm
6,600 rpm



&nbsp;
&nbsp;
&nbsp;


   Drivetrain
&nbsp;
&nbsp;



&nbsp;
&nbsp;


Drive configuration
Front engine/all-wheel drive


Transmission type
5-speed electronically controlled (Grade Logic) automatic overdrive transmission with manual shift mode



Traction Control System


Vehicle Dynamic Control (VDC) with cancel switch



&nbsp;
&nbsp;
&nbsp;


 Gear Ratio (:1)
  
&nbsp;


&nbsp;
&nbsp;
&nbsp;


Five-speed automatic
&nbsp;
&nbsp;


1 st
3.827
3.540


2 nd
2.368
2.264


3 rd
1.526
1.472


4 th
1.000
1.000


5 th
0.834
0.834


Reverse
2.613
2.370


Final drive ratio (:1)
3.692


Transfer gear ratio
1.000





&nbsp;



  Body, suspension and steering   



&nbsp;
&nbsp;
&nbsp;


Body type
Monocoque
&nbsp;


Front suspension
Independent strut with stabilizer bar


Rear suspension
Independent multi-link with stabilizer bar


Steering ratio (:1)
16.9
&nbsp;


Turning diameter (metres/feet)
11.8/38.7
&nbsp;


Turns (lock-to-lock)
2.7
&nbsp;


Steering type
Power-assisted rack-and-pinion





&nbsp;



 Brakes 



&nbsp;
&nbsp;
&nbsp;


Front:&nbsp;
Vented disc – 12.60" x 1.10"
&nbsp;


Rear: &nbsp;
Vented disc – 12.13" x 0.63"
&nbsp;



Electronic Brake force Distribution (EBD) and Brake Assist (BA)
&nbsp;


Four-channel/four-sensor Anti-lock Braking System (ABS)
&nbsp;





&nbsp;



    Electrical



&nbsp;
&nbsp;


Ignition system
Electronic


Alternator
110 amp


Battery
Low maintenance 80D23L 12-volt





&nbsp;



 Exterior dimensions(millimetres/inches)



&nbsp;
&nbsp;


Wheelbase
2850/112.2


Overall length
4803/189.1


Overall width w/mirrors folded
1925/75.8


Overall height
1674/65.9


Front track width
1593/62.7


Rear track width
1641/64.6


Minimum ground clearance
193/7.6


Coefficient of Drag (Cd)
0.35





&nbsp;



 Interior dimensions(millimetres/inches)



&nbsp;
Front 
 Rear 


Headroom
1006/39.6
998/39.3


Shoulder room
1445/56.9
1458/57.4


Hip room
1379/54.3
1397/55.0


Leg room
1115/43.9
894/35.2


Seating capacity
5
&nbsp;



Passenger volume (litres/cu.ft.)
2976/105.1


Cargo volume (litres/cu. ft)
776/27.4 /seats up, 1710/60.4 rear seats down


Total interior volume (litres/cu.ft)
3752/132.5


Fuel tank (litres)
90


Maximum towing capacity (kgs/lbs)
1588/3,500





&nbsp;



 Weight



&nbsp;
FX45
FX35 


Curb weight (kilos/lbs.)
1964/4330
1917/4226


Weight distribution (% fr/rr)
54/46
53/47


GVWR (lbs.)
2502/5515
2446/5,393





&nbsp;



   Fuel Economy (L/100km/mpg) 



&nbsp;
&nbsp;
&nbsp;


City
15.6/18
14.4/20


Highway
11.2/25
9.9/29



