2025 INFINITI QX50 Specifications




2025 INFINITI QX50 Specifications

January 30, 2025







Engine




&nbsp;






Type




KR20DDET






Camshaft design




DOHC






Configuration / Orientation




Transverse mounted






Cylinders / Configuration




4 / Inline






Block / Cylinder head composition




Aluminum / Aluminum






Displacement (l / cc)




2.0 litre/1,970 - 1,997 cc






Horsepower




268 hp @ 5,600 rpm






Torque (lb-ft)




280 lb-ft @ 1,600-4,800 rpm






Bore &amp; stroke (mm)




84.0 x 90.1 (8.0:1 CR) – 84.0 x 88.9 (14.0:1 CR)






Compression ratio (:1)




8.0 – 14.0 (variable)






Maximum engine speed (redline rpm)




6,000 rpm






Induction system




Turbocharged






Fuel delivery system




Direct and port injection






Valvetrain




4 valves per cylinder, 
Continuously Variable Valve Timing






Mounts




Front
Rear




2 solid (active control type)
2 liquid-filled, left and right side






Recommended fuel




Premium unleaded






Emission certification level




Tier3 Bin70/ LEV3-ULEV70






Exhaust




Dual system with sub and main mufflers






&nbsp;






Transmission and Drive System 




&nbsp;






Drive configuration




Intelligent all-wheel drive






Transmission type




Xtronic continuously variable transmission with manual shift mode and Downshift Rev Matching






CVT high ratio coverage (:1)




6.3






Reverse gear (:1)




0.745






Final drive (:1)




5.846






Vehicle Dynamic Control




S






Hill Start Assist




S






&nbsp;






Brakes 




&nbsp;






Front (in)




13.0-inch x 1.3-inch power-assisted vented disc






Rear (in)




12.1-inch x 0.6-inch power-assisted vented disc






Parking brake




Electronic, switch on console






Electronic brake force distribution




S






Anti-lock braking system






&nbsp;






Suspension and Steering 




QX50 PURE




QX50 SPORT




QX50 SENSORY






Body type




Corrosion-resistant and high-strength steel unibody construction, aluminum-alloy hood






Front suspension




MacPherson strut front suspension with aluminum-alloy upper and lower aluminum/steel subframe construction






Rear suspension




Independent multilink with stabilizer bar






Steering type




Speed-sensitive variable assist




S




S




S






Shock absorbers




Twin tube front, monotube rear






Steering ratio Rack EPS (:1)




15.3






Steering ratio DAS (:1)




13.1 - 21.1






Curb-to-curb turning circle diameter (ft)




36.4






&nbsp;






Exterior Dimensions (in/mm) 




&nbsp;






Wheelbase




110.2 in / 2,799.1 mm






Overall length




184.7 in / 4,691.38 mm






Overall width




74.9 in / 1,902.8 mm






Overall height




66.0 in / 1676.4 mm






Front track width




64.4 in / 1635.7 mm






Rear track width




19-inch wheels
20-inch wheels




64.2 in / 1630.7 mm
63.8 in / 1620.5 mm






Minimum ground clearance




8.6 in / 218.44 mm






Coefficient of drag (Cd)




0.32






Angle of approach (degrees)




17.2






Angle of departure (degrees)




23.9






Breakover angle (degrees)




19.0






Trunk liftover height




27.7 in / 703.58 mm






Step-in height, front/rear




17.2 in (436.88 mm) / 17.7 in (450.59 mm)






&nbsp;






Capacities &amp; Volume 






Seating capacity




5






Passenger compartment volume (litres)




1,503.8 w/moonroof, 1,540.6 w/o moonroof






Cargo volume with 2nd row up (litres)




880.1 w/moonroof, 888.6 w/o moonroof






Cargo volume with 2nd row folded (litres)




1,822.5 w/moonroof, 1,842.3 w/o moonroof






Total interior volume (litres)




3,772.4 w/moonroof, 3,843.1 w/o moonroof






Fuel tank (litres)




60






Engine oil (litres)




4.7






Engine coolant (litres)




7.7






&nbsp;






Interior Dimensions (mm) 






Headroom




&nbsp;






&nbsp;




Front seats (without moonroof)




1,016 (1,041.4)






&nbsp;




Rear seats (without moonroof)




975.36 (993.14)






Legroom




&nbsp;






&nbsp;




Front seats




1,005.8






&nbsp;




Rear seats




983






Shoulder room




&nbsp;






&nbsp;




Front seats




1,470.7






&nbsp;




Rear seats




1,450.34






Hip room




&nbsp;






&nbsp;




Front seats




1,412.2






&nbsp;




Rear seats




1,366.52






&nbsp;






Wheels and Tires 




QX50 PURE 




QX50 SPORT 




QX50 SENSORY 






19 x 7.5-inch aluminum-alloy wheels




S




-




-






20 x 8.5-inch aluminum-alloy wheels (silver painted and machine finished)




-




-




S






20 x 8.5-inch aluminum-alloy wheels (black painted and machine finished)




-




S




-






All-season, run-flat P235/55R19 tires




S




-




-






All-season, run-flat P255/45R20 tires




-




S




S






Tire pressure monitoring system-Direct sensor type




S






Easy fill tire alert




S






&nbsp;






Exterior Features and Options 




QX50 PURE 




QX50 SPORT 




QX50 SENSORY 






LED headlights (low/high beam)




S






Unique cube design headlights




-




-




S






LED signature daytime running lights




S






Front LED fog lights




S


&nbsp;






Adaptive Front lighting System




-




-




S






LED Taillights




S






Body-colour outside mirrors




S




-




S






Black outside mirror caps




-




S




-






Power, auto folding outside mirrors




-




S




S






Heated outside mirrors




S


&nbsp;






Reverse tilt-down mirrors




-




S




S






Panoramic moonroof with power open/tilt and power sunshade




-




S




S






Aluminum roof rails




-




S




S






Body-coloured door handles with chrome accent and welcome LED light




S




-




S






Body-coloured door handles and welcome LED light




-




S




-






UV-reducing, noise-insulated windshield




S






Power liftgate




S






Motion-activated liftgate




-




S




S






&nbsp;




&nbsp;




&nbsp;




&nbsp;






Black mesh grille and front grille surround




-




S




-






Black front fender accent




-




S




-






Black liftgate finisher




-




S




-






Body color rear diffuser




-




S




-






Exclusive I-LINE badge




-




S




-






&nbsp;






Audio and Infotainment 




QX50 PURE 




QX50 SPORT 




QX50 SENSORY 






INFINITI InTouch™ dual HD display system with LCD/VGA 8.0-inch upper and 7.0-inch lower touchscreens




S






INFINITI InTouch™ Services telematics with four year Premium package included




S






Siri® Eyes Free




S






Wireless Apple CarPlay® integration




S






Android Auto™ integration




S






Six-speaker audio system




S




-




-






Bose® 12-speaker premium audio




&nbsp;




S




&nbsp;






Bose® Performance Series Audio 16-speaker audio with Bose® Audio Pilot 2 and Bose® CenterPoint® 2 technology




-




-




S






Head-up display




-




-




S






HD Radio® Technology




S






Streaming audio via Bluetooth®




S






Voice Recognition




S






SiriusXM® Radio (Subscription 
required, sold separately)




S






Wi-Fi hotspot (Subscription 
required, sold separately)




S






Five USB connection ports (three Type-A, two Type-C)




S






Navigation with detailed real time Premium Traffic info, 3D building graphics, &amp; seamless turn-by-turn directions, SiriusXM® Travel Link and SiriusXM® Traffic




-




S




S






&nbsp;






Safety, Security and 
Driver-Assist Features 




QX50 PURE 




QX50 SPORT 




QX50 SENSORY 






INFINITI Advanced Air Bag System




S






Rear seat-mounted side-impact supplemental air bags




S






3-point ALR/ELR (driver ELR only) front seat belts with pretensioners and load limiters and adjustable upper anchors




S






3-point rear seat belts (ALR/ELR all positions)




S






Forward Emergency Braking with pedestrian detection




S






Predictive Forward Collision Warning




S






Lower Anchors &amp; Tethers for Children (LATCH)




S






INFINITI Vehicle Immobilizer System




S






RearView Monitor




S


&nbsp;






Around View Monitor® with Moving Object Detection




-




S




S






Blind Spot Warning and Intervention




S






Lane Departure Warning and Intervention




S






ProPILOT Assist




S






Intelligent Cruise Control with Full Speed Range




S






High Beam Assist




S






Traffic Sign Recognition




-




S




S






Rear Automatic Braking




S


&nbsp;






Rear Cross Traffic Assist




S






Vehicle Dynamic Control (VDC) with Traction Control System




S






&nbsp;






Curb Weights (kg) 




QX50 PURE 




QX50 SPORT  




QX50 SENSORY 






AWD




AWD




AWD






Front 
Rear
Total




1070
736
1806




1089
787
1876




1090
788
1878






Weight distribution 
(% FR/RR, with driver)




60 / 40




60 / 40




60 / 40






GVWR




2302




2302




2302






&nbsp;






NRCAN Fuel Economy (L/100km) 




QX50 AWD 






City
Highway
Combined




10.8
8.3
9.7






&nbsp;


# # #
